Foundation Inspection Checklist
REI Grid
Spot foundation red flags (especially Texas expansive soils)
Template for reference and customization only. Not legal, tax, or financial advice. Laws and requirements vary by state and locality — consult a licensed professional and verify your jurisdiction’s rules before use.
	Property address: ______________________
	Date: ______________________

	Inspected by: ______________________
	


Look for
☐  Exterior cracks in brick / stucco (stair-step cracks)
☐  Interior wall & ceiling cracks (corners of doors/windows)
☐  Doors & windows sticking or out of square
☐  Sloping / uneven / bouncy floors
☐  Gaps at trim, cabinets, or where walls meet ceiling
☐  Separation of brick from windows / soffit
☐  Drainage & grading slope away from foundation
☐  Gutters & downspouts direct water away
☐  Large trees / roots near the foundation
☐  Evidence of prior foundation repair (warranty?)
☐  Signs of plumbing leaks under slab (high bills, warm floors)
Texas note: expansive clay soils make foundation movement common. If multiple items are flagged, obtain an evaluation from a licensed structural / foundation engineer before proceeding.
Overall assessment:  __________________________________________________
Engineer evaluation recommended? (Y/N):  __________________________________________________
REI Grid  ·  Foundation Inspection Checklist  ·  Template v1.0  ·  For reference only — not legal, tax, or financial advice  ·  Page 
